{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["询比清单8月4日"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询比清单8月4日","index":0,"n_rows":9,"n_cols":8,"rows_kept":9,"merged":[[0,0,0,7],[1,0,1,7],[5,0,5,7],[6,0,6,7],[7,0,7,7],[8,0,8,7]],"flags":["formulas_cached_only"]}
["陕西锌业有限公司"]
["智能超声波探伤仪询比采购报价单"]
[" 序号","物资名称","厂家品牌","规格型号","数量","单位","单价（元）","金额（元）"]
[1,"智能超声波探伤仪",null,"JITAI1991，                                                          扫描范围： 0~6000MM钢纵波 \n脉冲强度： 可调 \n工作频率： 0.4MHZ~20MHZ \n垂直线性误差： ≤3% \n水平线性误差： ≤0.1% \n增益：120DB \n灵敏度余量： >62DB(深200MMΦ2平底孔) \n分辨力：>40DB(5N20) \n探头阻尼：50Ω~400Ω多个档位可调 \n动态范围： ≥32DB \n电噪声电平：<8% \n硬采样频率：320MHZ \n重复发射频率：100~1000HZ \n声速范围：100-15000(M/S) \n工作方式：单品直探头探伤、单晶斜探头探伤，双晶探伤、穿透探伤 \n要求：仪器自带第三方检定报告",1,"台"]
["合计"]
["报价单填写说明：竞价方在报价栏填报单价，合计金额，厂家品牌必须注明，填好的报价单由公司法定代表人或授权委托人签名并加盖公司公章，（扫描件、电子版、上传竞价平台作为正式报价）。"]
["           报价单位：（章） "]
["                             法定代表人或授权委托人：      （签名）   "]
["                    报价时间：   年     月   日                                           "]